**Information Sheet 1**

## PLANER SAFETY RULES

1. Follow all General Shop Safety Rules.
2. Be sure stock is free from metal, paint, or other foreign materials. ABSOLUTELY NO USED LUMBER IS TO BE RUN THROUGH THE PLANER.

3. Do not surface stock shorter than 13”.

4. Do not look into the machine while it is running.

5. Do not stand directly behind any stock that is being surfaced.

6. Feed stock into the machine so that it is flat on the table. Never allow your fingers to get between the stock and the table surface.

7. Do not attempt to take more than 1/8” per cut with 1/16” being the normal amount of stock removal.

8. When surfacing stock of uneven thickness, adjust the machine to the maximum thickness of the stock for the first pass, and reduce accordingly for successive passes.