**Information Sheet 2**

## GRAIN DIRECTION DIAGRAM

# The cutter-head of the planer is above the wood, exactly the opposite of a jointer, where the cutter-head is below the wood. When machining wood with a planer, the grain direction must be correctly oriented to minimize tear-out.

# 

# 