## Skill Activity 1

### PARTS & ADJUSTMENT FOR FESTOOL CIRCULAR SAW

|  |  |
| --- | --- |
| Completed | Procedure |
| □ | 1. Obtain a Festool Track Saw and a portable circular saw. Use the labeled diagrams or tool manuals to locate the following parts of the tools: trigger switch, height adjustment knob, tilt scale, tilt lock knob, blade, blade guard (retractable), tilting base, line-of-sight cutting guide, guard lift handle.
 |
| □ | 1. Adjust blade for a 2” deep cut. (Saw NOT plugged in.)
 |
| □ | 1. Adjust blade to a 15 degree bevel. Check it with a T-bevel set to 75 degrees on a protractor. (Saw NOT plugged in.)
 |
| □ | 1. Return blade to 0 degrees. Follow the procedure on the Blade Changing Instruction sheet to remove and replace the blade. Make sure you install the blade with the teeth in the right direction.
 |
|  |  |