
**Ex. 6.1 - Fixed Spindle Shaper Drawing & Evaluation**



**Scoring Guide:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Straight Bead is centered on stock | Curved Bead is centered on stock and blends with straight bead | Cove #1 is centered on the stock | Cove #2 is centered on the stock | Accuracy of Part dimensions |
| Quality of straight bead | Quality of curved bead; No overcut from band saw | Quality of Cove #1 | Quality of Cove #2 | All operations complete on 1 piece |

Dimensional Accuracy +/- 1/64" Quality = no tearout or burning

Minimum passing score: 8/10 Total Points \_\_\_\_\_\_\_\_\_\_\_\_

Comments: Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_