## **Skill Activity 2**

## **RIPPING AND RE-SAWING**

|  |  |
| --- | --- |
| **Completed √** | **Procedure** |
| □  □  □  □  □ | 1. Review the Band Saw safety rules. 2. Obtain 2 pieces of ¾” x 3” x 15-1/2” stock. 3. Lay out a straight line along one edge half the thickness of the stock. Using a pivot block, lower the blade guide to the proper position, and resaw the stock on the line. 4. Use one of the cut pieces to test for and align a straight fence for drift. 5. Place the fence in position, either inside or outside the blade, and resaw piece B exactly in half. Use a push stick to feed the work through the saw. Hold the stock against the fence with a support block.   -------------------------------------------------------------------------------- |